HFS Prices June 1 2019 

A Gen 20 system is lighter , more compact and more energy efficient and more advanced than a Gen 15 systems and are used for engines greater than 8 litre capacity

Gen 15 systems are able to be used instead of Gen 20 systems up to 8 litre engine capacity. Latest Model Gen 15 system is great producer as is Gen 20 . Gen 15 system fully welded SS316L and heavier than Gen 20

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| SYSTEM | vehicle | Weight | Plate area | Price  | Enclosure | Engine fuel |
| Gen 10 system | family cars to 4 litre capacity | 14.5 kg | 6400 sq cm | POA | Aluminum43cm x 25 cm x 33 cm high | Petrol , diesel, LPG |
| Gen 10 system | family cars to 4 litre capacity | 15.5 kg | 6400 sq cm | POA | Steel43cm x 25 cm x 33 cm high | Petrol , diesel, LPG |
| Gen 10 system | family cars to 4 litre capacity | 13.5 kg | 6400 sq cm | POA | Plastic40 cm x 20 cm x 27 cm high | Petrol , diesel, LPG |
| Gen 15 | Vehicles/ trucks/ 4 WD work vehicles  engine capacity greater than 4 litre | 19.5 kg | 14400 sq cm | POA | Steel43  cm x 25 cm x 37 cm high | Petrol , diesel, LPG |
| Gen 15 | Vehicles/ trucks/ 4 WD work vehicles  engine capacity greater than 4 litre | 15.5 kg | 14400 sq cm | POA | Aluminum43  cm x 25 cm x 37 cm high | Petrol , diesel, LPG |
| Gen 20 | Trucks/ Gensets / Trawlers  engine capacity greater than 4 litre | 14kg | 8400 sq cm | POA | Plastic35  cm x 40 cm x 30 cm high | Petrol , diesel, LPG |
| Gen 20 | Trucks/ Gensets / Trawlers  engine capacity greater than 4 litre | 19kg | 8400 sq cm | POA | Steel35 cm x 40 cmx33cm high | Petrol , diesel, LPG |
| Gen 20 | Trucks/ Gensets / Trawlers  engine capacity greater than 4 litre | 15kg | 8400 sq cm | POA | Checker-plate aluminum35  cm x 40 cm x 33 cm high | Petrol , diesel, LPG |
| Gen 30 | Trucks/ Gensets / Trawlers  engine capacity greater than 30 litre | 400 kg | 105000 sq cm | POA | Steel  | Petrol , diesel, LPG |

|  |  |  |
| --- | --- | --- |
| ENGINE CAPACITY  | Gen 10 Hydrogen system | Gen 15 Gen 20 Hydrogen system |
| Up to 3 litre | One Gen 10 |  |
| Up to 4 litre | One Gen 10  |  |
| 5 litre |  | One Gen 15 or Gen 10 |
| 6 litre  |  | One Gen 15 |
|  7 litre |  | One Gen15 |
| 8 litre |  | One Gen 15 |
| 9 litre |  | One Gen 15 or Gen 20 |
| 10 litre |  | Two Gen 15 or Gen 20 |
| 11 litre |  | Two Gen 15 or Gen 20 |
| 12 litre |  | Two Gen 15 or Gen 20 |
| 13 litre |  | Two Gen 15 or Gen 20 |
| 14 litre |  | Two Gen 15 or Gen 20 |
| 15litre |  | Two Gen 15 or Gen 20 |
| 16 litre |  | Two Gen 15 or Gen 20 |
| 17 litre |  | Three Gen 15 or Gen 20 |
| 18 litre |  | Three Gen 15 or Gen 20 |
| 19 litre |  | Three Gen 15 or Gen 20 |
| 20 litre |  | Three Gen 15 or Gen 20 |